# Digital Eagle QR-07S3

Technical Documents

**Digital Eagle QR-07S3 Hand Gun portable jamming system**

**Applications:**
Prevent remote controlled improvised explosive devices from being activated and stop terrorist attacks;
Protect explosives handling experts;
Protect important places such as bus/train stations, plazas, schools, mass gatherings, stadiums, etc;
Risk mitigation and explosives removal in specified spots;
Police used for VVIP convoy, ECM, anti drug, riot control, etc.
Military used for border control, ECM etc.

**Features:**

* **Handgun with adjustable armrest**
* It can be operated by one (1) person in less than three minutes
* Lightweight system with a total weight of less than 20 kg.
* Effective range of 1500 m.

**Technical Parameters**

|  |  |  |  |
| --- | --- | --- | --- |
| **Brand** | Digital Eagle | **Model** | QR-07S3 |
| **Reference** | Hand Gun portable jamming system | **Control unit** | Internal, integrated with body |
| **Package** | Kitboxinternal part has high density polyurethane foamexternal case with wheels | **Weight with box** | 9kg |
| **Dimensions** | 746\*228\*79mm | **Weight with battery** | 4kg |
| **Operation Frequency** | 832-932MHz,2.4GHz, 5.8GHz, GPS, GLONASS, GALILEO L1 | **Antenna** | Directional Antenna |
| **Effective range** | 1500m | **Type of operation** | Blocker operating frequencies, manual action. |
| **Jamming type** | Lock and block operation and transmission and navigation of UAV.1. RTH
2. Landing immediately
 | **Control of output power** | Adjustable 2 levels |
| **Working time** | 60mins | **Battery**  | 2pcs of rechargeable lithium batteries |
| **Standby times** | 24hrs | **Battery charger** | Customized for all countries |
| **Operation temperature**  | -25℃~+60℃ | **Warranty** | 1 year |

**Packing List**

1. Drone Jammer Gun\*1
2. Telescope\*1
3. High capacity Lithium battery\*2
4. Battery charger\*1
5. Restraint harness the rifle \*1
6. Tripod\*1
7. Anti-shake ,Anti-dust, waterproof carrying case\*1