# Digital Eagle QR-09

Technical Documents

**Digital Eagle QR-09 Fixed jamming system**

**Applications:**
Prevent remote controlled improvised explosive devices from being activated and stop terrorist attacks;
Protect explosives handling experts;
Protect important places such as bus/train stations, plazas, schools, mass gatherings, stadiums, etc;
Risk mitigation and explosives removal in specified spots;
Police used for VVIP convoy, ECM, anti drug, riot control, etc.
Military used for border control, ECM etc.

**Features:**

* Non-invasive Fixed jamming system
* It can be operated by one (1) person in less than three minutes

**Technical Parameters**

|  |  |  |  |
| --- | --- | --- | --- |
| **Brand** | Digital eagle | **Model** | QR-09 |
| **Reference** | Fixed jamming system | **Operation** | Operated by 1 person |
| **Dimensions** | 820\*540\*360mm | **Weight**  | 20kg |
| **Operation Frequency** | 2.4GHz, 5.8GHz, GPS, GLONASS, GALILEO L1 | **Antenna** | Directional Antenna &Omni antenna |
| **Effective range** | Omni:500mDirectional:1500m | **Type of operation** | Blocker operating frequencies |
| **Jamming type** | Lock and block operation and transmission and navigation of UAV.1. RTH
2. Landing immediately
 | **Control of output power** | Adjustable 2 levels |
| **Working time** | 24hrs\*7 | **Power source** | AC input |
| **AC input voltage** | Customized for all countries | **Warranty** | 1 year |
| **Operation temperature**  | -25℃ ~ +60℃ | **Wheel case** | Yes |
| **Control Panel** | Integrated with main body |